PRESENTATION SWITCHERS (DVX-2255HD-T)

1) 용  도

본 기기는 HDMI, DVI, DXLink, Audio 신호를 수용할 수 있는 통합 오디오, 비디오 제어 장치로서 스케일러, 아날로그-디지털 신호 변환, 오디오 프로세싱과 같은 다양한 기능을 통합하고 소스와 디스플레이가 서로 다른 해상도를 가질 때 발생할 수 있는 문제를 제거해 준다. 또한 전용 프로토콜 케이블을 통한 동일 제조사의 확장성이 매우 뛰어나며, 크고 복잡한 회의실, 강의실 및 강당에 간편하게 설치 할수 있다.

2) 기  능

- 올인원 기기

- 단순성 및 신뢰성 제공

- 총 소유 비용 (TCO) 절감

- 독보적인 네트워크 보안

- 최적의 비디오 이미지 품질

- 오디오 매트릭스 스위칭

- 향상된 마이크 프로세싱

- 매트릭스 스위칭

- AV 및 컨트롤

- HDMI / HDCP 스위칭

- 멀티 포맷 포트

- DXLink ™ 트위스트 페어 출력

- SmartScale 기술 내장

3) 사  양

- HDMI Input Port : 2 Port

- DVI Input Port : 2 Port

- HDMI output Port : 2 Port

- Audio Input Port : 2 Port (1/8" stereo mini-phono jacks)

: 2 Port (5-position captive-wire terminals)

: 2 Port (3-pin captive-wire MIC connectors)

- Audio output Port : 1 Port (Amplified), 2 Port (Line level)

- S/PDIF output Port : 1 Port

- RS-232/422/485 Port : 1 Port

- RS-232 Port : 3 Port

- IR/Serial : 4 Port

- I/O Channels : 1 Port

- Ethernet : Ethernet, ICS lan

- Relay : 4 Port

- NVRAM : 1 MB

- Memory Card : 16 GB SD

- DDRAM : 1 GB

- Link port : DX Link(in)(2), DX Link(out)(1), AX Link(1)

- Processor : 1600MIPS

- Power Consumption : 80 W (typical)

: 85 to 90 W (typical average)

: 30 W (typical in low-power mode)

- Amplifier : 75W, 70V / 100V

- Dimension (H x W x D)mm : 132 x 432 x 356

- Weight : 8.26 kg