DVI OUTPUT BOARD (DGX-O-DVI)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 HDCP 규격을 준수하는 DVI 출력 보드로서, 4개의 DVI 커넥터가 지원되며 HDMI 혹은 DVI 신호 출력을 지원한다. 전용 SmartScale® 스케일링 기술을 통해 서로 다른 해상도의 여러 디스플레이에 최적화된 해상도로 스케일링을 지원한다.

2) 기  능

- InstaGate Pro® HDCP 인증키 기술

- SmartScale - 디스플레이 별 최적 자동 스케일링

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 음원 지원 (Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, and 2-channel through 8-channel L-PCM)

3) 사  양

DVI w/HDCP

- Compatible Formats: DVI, HDCP

- Signal Type Support:

DVI-D (Single Link)

HDMI (With DVI Cable Adapter)

HDMI Mode Support: DVI boards can be run in HDMI mode with an EDID update which will provide full HDMI functionality and board specifications

- Data Rate (Max): 4.95 Gbps

- Pixel Clock (Max): 165 MHz

- Progressive Resolution Support: 480p up to 1920x1200 @ 60 Hz

If input is interlaced, all scaled outputs will deinterlace video to a progressive resolution format. If in scaler Bypass mode interlaced input will pass through unaltered

- Interlaced Resolution Support: 480i, 576i, 1080i

- 2K Resolution Support: 2048x1024 @ 47Hz, 2048x1080 @ 60Hz, 2048x1152 @ 60Hz, 2048x1536 @ 24Hz

2K formats are only compatible with the DVI and HDMI Input/Output boards and require the output scaler to be set in Bypass mode

- Output Re-clocking: Yes

- Output Scaling: SmartScale or manual configuration or Bypass

- SmartScale Output Resolution Support: All resolutions between 480p and 1920 x 1200 @ 60 Hz via automatic SmartScale query of the display's declared EDID Detailed Timing Definition.

- Color Depth Support: 24-bit

- Color Space Support: RGB 4:4:4

- Local Audio Support: Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel

- DDC/EDID Support: EDID provided by Enova DGX 8 / 16 / 32 / 64

EDID is user re-programmable

- HDCP Support: Yes, full matrix HDCP support (includes any input to any or all outputs)

Key Management System

- AMX HDCP InstaGate Pro Technology: Key support up to 16 devices per output, independent of source device

- Output Voltage (Nominal): 1.0 Vpp Differential

Output Rise Time / Fall Time:

100 ps min - 200 ps max (20% - 80%)

0.16 UI min - 0.33 UI max (@ 1.65 Gbps, 20% - 80%)

- Output +5V DDC Pin: 50 mA

- DVI Output Board Propagation Delay: 24 ms for progressive, 48 ms for interlace, 5 us when in Bypass mode

- Connectors: 4 DVI-I Ports, (DVI-D Single Link is the supported signal type)