HDMI INPUT BOARD (DGX-I-HDMI)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 HDMI 입력 보드이며, 4개의 HDMI 포트가 오디오, 비디오 신호 전송을 지원한다.

2) 기  능

- InstaGate Pro® HDCP 인증키 기술

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 오디오 지원

3) 사  양

HDMI w/HDCP

- Compatible Formats: HDMI, HDCP, DVI

Signal Type Support:

HDMI

DVI-D (Single Link With HDMI Cable Adapter)

DisplayPort ++ (Input Only, With HDMI Cable Adapter)

- Video Data Rate (Max):

4.95 Gbps / 6.75 Gbps

6.75 Gbps supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Video Pixel Clock (Max):

165 MHz / 225 MHz

225 MHz supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Progressive Resolution Support: 480p up to 1920x1200 @ 60 Hz

- Interlaced Resolution Support:

480i, 576i, 1080i

If input is interlaced, all scaled outputs will deinterlace video to a progressive resolution format. If in scaler Bypass mode interlaced input will pass through unaltered

- 2K Resolution Support: 2048x1024 @ 47 Hz, 2048x1080 @ 60 Hz, 2048x1152 @ 60 Hz, 2048x1536 @ 24 Hz

- Input Equalization: Yes, Adaptive up to 100ft (30m) at 225 MHz, Cable distance support dependent on cable type and signal format

- Input Re-clocking (CDR): Yes

- Deep Color Support:

24-bit, 30-bit, 36-bit

30-bit, 36-bit supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Color Space Support:

RGB 4:4:4

YCbCr 4:4:4 and 4:2:2

Input signal support for YCbCr 4:4:4 and 4:2:2, output color-space is converted to RGB 4:4:4

- 3D Format Support:

Yes (HDMI Primary Formats)

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/6 0Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

3D supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192 kHz

- Local Audio Support: Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel

- DDC/EDID Support:

EDID provided by Enova DGX 8/ 16 / 32 / 64

EDID is user re-programmable

- HDCP Support: Yes, full matrix HDCP support (includes any input to any or all outputs)

Key Management System:

AMX HDCP InstaGate Pro Technology

Key support up to 16 devices per output, independent of source device

CEC Support: None

Input Voltage (Nominal): 1.0 Vpp Differential

Connectors: 4 HDMI Type A Female Ports

HDMI Input Board Propagation Delay: 2 us

HDMI Audio Synchronization:

Progressive and Interlace Video Formats @ 60 Hz frame rate: Audio is actively delayed to match video within 8ms leading or lagging