6-BUTTON KEYPAD (MKP-106L-WH)

1) 용  도

본 기기는 6-버튼 키패드이며 컨트롤러가 제외된 모델으로 스타일리쉬한 디자인에 심플한 컨트롤을 제공하며 이더넷으로 간편하게 연결하여 호환 통합제어 기기와 사용할 수 있다.

2) 기  능

- 스탠더드 이더넷 프로토콜 지원 및 PoE

- 6채널 버튼 및 LED 피드백

3) 사  양

DIMENSIONS (HWD)

- Portrait: 4 11/16" x 3 7/16" x 9/16" (119 mm x 87.5 mm x 13.9 mm)

- Landscape: 3 7/16" x 4 11/16" x 9/16" (87.5 mm x 119 mm x 13.9 mm)

- WEIGHT: Approximately .25 lbs (.11 kg)

POWER CONSUMPTION

- Typical: 4.5 Watts

- Voltage, DC (Typical): PoE (37V-57V)

- Voltage DC Range: 37 V-57 V per 802.3af spec

- Power Connector: (1) RJ-45 Ethernet

POWER SUPPLY

- External, Required: Any POE injector or switch, conforming to the 802.3af standard including AMX’s PS-POE-AF-TC (FG423-83), not included

ENVIRONMENTAL

- Temperature (Operating): 32° F to 122° F (0° C to 50° C)

- Temperature (Storage): 14° F to 140° F (-10° C to 60°C)

- Humidity (Operating): 5% to 85% RH

ETHERNET

- Ethernet Connection: (1) 10/100; Port provides TCP/IP communication. This is an Auto MDI/MDI-X enabled port, which allows you to use either straight-through or crossover Ethernet cables. The Ethernet Port LEDs show communication activity, connection status, speeds, and mode information.

CONTROL PORTS & INDICATORS

- Program Port: (1) USB Mini-B, USB

- ID Pushbutton: Reset factory settings, reset factory image, toggle between DHCP or static IP addressing mode

MEMORY

- Flash: 4 GB

- Memory Card: 4 GB SD

- DDRAM: 256 MB

- REGULATORY COMPLIANCE

FCC CFR Title 47 Part 15

CE EN 55022

CE EN 55024

CE EN 60950-1

IEC 60950-1

UL 60950-1

C-Tick CISPR 22

IC CISPR 22

VCCI CISPR 22

RoHS

WEEE

GENERAL

- Mounting Options: Mount onto standard 1 gang US, UK, or EU back boxes

- Front Panel Components: 6 Buttons

- Color / Styles Available:

Portrait, Black: MKP-106P-BL (FG1313-06P-B)

Portrait, White: MKP-106P-WH (FG1313-06P-W)

Landscape, Black: MKP-106L-BL (FG1313-06L-B)

Landscape, White: MKP-106L-WH (FG1313-06L-W)